(module molex_impact_85ohm_left_and_right_guided_240pin_0.39mm (layer F.Cu) (tedit 605E9B45)
  (descr "Impact 85 Ohm Plus 4 Pair Vertical Header, Right Guided, Left Endwall, 10 Columns, 120 Circuits, Pin Length 4.90mm, Plated Through Hole Dimension 0.39mm, Lead Free")
  (fp_text reference REF** (at 26.55 -21.8) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value molex_impact_85ohm_left_and_right_guided_240pin_0.39mm (at 26.55 -1.2) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 0 0) (end 0 -20.8) (layer F.SilkS) (width 0.12))
  (fp_line (start 0 -20.8) (end 53.1 -20.8) (layer F.SilkS) (width 0.12))
  (fp_line (start 53.1 -20.8) (end 53.1 0) (layer F.SilkS) (width 0.12))
  (fp_line (start 53.1 0) (end 0 0) (layer F.SilkS) (width 0.12))
  (fp_line (start 0 0) (end 0 -20.8) (layer F.CrtYd) (width 0.05))
  (fp_line (start 0 -20.8) (end 53.1 -20.8) (layer F.CrtYd) (width 0.05))
  (fp_line (start 53.1 -20.8) (end 53.1 0) (layer F.CrtYd) (width 0.05))
  (fp_line (start 53.1 0) (end 0 0) (layer F.CrtYd) (width 0.05))
  (pad 1 thru_hole rect (at 8.5 -17.825) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 2 thru_hole circle (at 8.5 -16.475) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 3 thru_hole circle (at 8.5 -15.125) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 4 thru_hole circle (at 8.5 -13.775) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 5 thru_hole circle (at 8.5 -12.425) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 6 thru_hole circle (at 8.5 -11.075) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 7 thru_hole circle (at 8.5 -9.725) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 8 thru_hole circle (at 8.5 -8.375) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 9 thru_hole circle (at 8.5 -7.025) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 10 thru_hole circle (at 8.5 -5.675) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 11 thru_hole circle (at 8.5 -4.325) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 12 thru_hole circle (at 8.5 -2.975) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 13 thru_hole circle (at 10.4 -17.825) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 14 thru_hole circle (at 10.4 -16.475) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 15 thru_hole circle (at 10.4 -15.125) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 16 thru_hole circle (at 10.4 -13.775) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 17 thru_hole circle (at 10.4 -12.425) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 18 thru_hole circle (at 10.4 -11.075) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 19 thru_hole circle (at 10.4 -9.725) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 20 thru_hole circle (at 10.4 -8.375) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 21 thru_hole circle (at 10.4 -7.025) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 22 thru_hole circle (at 10.4 -5.675) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 23 thru_hole circle (at 10.4 -4.325) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 24 thru_hole circle (at 10.4 -2.975) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 25 thru_hole circle (at 12.3 -17.825) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 26 thru_hole circle (at 12.3 -16.475) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 27 thru_hole circle (at 12.3 -15.125) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 28 thru_hole circle (at 12.3 -13.775) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 29 thru_hole circle (at 12.3 -12.425) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 30 thru_hole circle (at 12.3 -11.075) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 31 thru_hole circle (at 12.3 -9.725) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 32 thru_hole circle (at 12.3 -8.375) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 33 thru_hole circle (at 12.3 -7.025) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 34 thru_hole circle (at 12.3 -5.675) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 35 thru_hole circle (at 12.3 -4.325) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 36 thru_hole circle (at 12.3 -2.975) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 37 thru_hole circle (at 14.2 -17.825) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 38 thru_hole circle (at 14.2 -16.475) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 39 thru_hole circle (at 14.2 -15.125) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 40 thru_hole circle (at 14.2 -13.775) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 41 thru_hole circle (at 14.2 -12.425) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 42 thru_hole circle (at 14.2 -11.075) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 43 thru_hole circle (at 14.2 -9.725) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 44 thru_hole circle (at 14.2 -8.375) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 45 thru_hole circle (at 14.2 -7.025) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 46 thru_hole circle (at 14.2 -5.675) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 47 thru_hole circle (at 14.2 -4.325) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 48 thru_hole circle (at 14.2 -2.975) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 49 thru_hole circle (at 16.1 -17.825) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 50 thru_hole circle (at 16.1 -16.475) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 51 thru_hole circle (at 16.1 -15.125) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 52 thru_hole circle (at 16.1 -13.775) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 53 thru_hole circle (at 16.1 -12.425) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 54 thru_hole circle (at 16.1 -11.075) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 55 thru_hole circle (at 16.1 -9.725) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 56 thru_hole circle (at 16.1 -8.375) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 57 thru_hole circle (at 16.1 -7.025) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 58 thru_hole circle (at 16.1 -5.675) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 59 thru_hole circle (at 16.1 -4.325) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 60 thru_hole circle (at 16.1 -2.975) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 61 thru_hole circle (at 18 -17.825) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 62 thru_hole circle (at 18 -16.475) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 63 thru_hole circle (at 18 -15.125) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 64 thru_hole circle (at 18 -13.775) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 65 thru_hole circle (at 18 -12.425) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 66 thru_hole circle (at 18 -11.075) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 67 thru_hole circle (at 18 -9.725) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 68 thru_hole circle (at 18 -8.375) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 69 thru_hole circle (at 18 -7.025) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 70 thru_hole circle (at 18 -5.675) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 71 thru_hole circle (at 18 -4.325) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 72 thru_hole circle (at 18 -2.975) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 73 thru_hole circle (at 19.9 -17.825) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 74 thru_hole circle (at 19.9 -16.475) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 75 thru_hole circle (at 19.9 -15.125) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 76 thru_hole circle (at 19.9 -13.775) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 77 thru_hole circle (at 19.9 -12.425) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 78 thru_hole circle (at 19.9 -11.075) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 79 thru_hole circle (at 19.9 -9.725) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 80 thru_hole circle (at 19.9 -8.375) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 81 thru_hole circle (at 19.9 -7.025) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 82 thru_hole circle (at 19.9 -5.675) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 83 thru_hole circle (at 19.9 -4.325) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 84 thru_hole circle (at 19.9 -2.975) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 85 thru_hole circle (at 21.8 -17.825) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 86 thru_hole circle (at 21.8 -16.475) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 87 thru_hole circle (at 21.8 -15.125) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 88 thru_hole circle (at 21.8 -13.775) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 89 thru_hole circle (at 21.8 -12.425) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 90 thru_hole circle (at 21.8 -11.075) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 91 thru_hole circle (at 21.8 -9.725) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 92 thru_hole circle (at 21.8 -8.375) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 93 thru_hole circle (at 21.8 -7.025) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 94 thru_hole circle (at 21.8 -5.675) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 95 thru_hole circle (at 21.8 -4.325) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 96 thru_hole circle (at 21.8 -2.975) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 97 thru_hole circle (at 23.7 -17.825) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 98 thru_hole circle (at 23.7 -16.475) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 99 thru_hole circle (at 23.7 -15.125) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 100 thru_hole circle (at 23.7 -13.775) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 101 thru_hole circle (at 23.7 -12.425) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 102 thru_hole circle (at 23.7 -11.075) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 103 thru_hole circle (at 23.7 -9.725) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 104 thru_hole circle (at 23.7 -8.375) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 105 thru_hole circle (at 23.7 -7.025) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 106 thru_hole circle (at 23.7 -5.675) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 107 thru_hole circle (at 23.7 -4.325) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 108 thru_hole circle (at 23.7 -2.975) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 109 thru_hole circle (at 25.6 -17.825) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 110 thru_hole circle (at 25.6 -16.475) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 111 thru_hole circle (at 25.6 -15.125) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 112 thru_hole circle (at 25.6 -13.775) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 113 thru_hole circle (at 25.6 -12.425) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 114 thru_hole circle (at 25.6 -11.075) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 115 thru_hole circle (at 25.6 -9.725) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 116 thru_hole circle (at 25.6 -8.375) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 117 thru_hole circle (at 25.6 -7.025) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 118 thru_hole circle (at 25.6 -5.675) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 119 thru_hole circle (at 25.6 -4.325) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 120 thru_hole circle (at 25.6 -2.975) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 121 thru_hole circle (at 27.5 -17.825) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 122 thru_hole circle (at 27.5 -16.475) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 123 thru_hole circle (at 27.5 -15.125) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 124 thru_hole circle (at 27.5 -13.775) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 125 thru_hole circle (at 27.5 -12.425) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 126 thru_hole circle (at 27.5 -11.075) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 127 thru_hole circle (at 27.5 -9.725) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 128 thru_hole circle (at 27.5 -8.375) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 129 thru_hole circle (at 27.5 -7.025) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 130 thru_hole circle (at 27.5 -5.675) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 131 thru_hole circle (at 27.5 -4.325) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 132 thru_hole circle (at 27.5 -2.975) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 133 thru_hole circle (at 29.4 -17.825) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 134 thru_hole circle (at 29.4 -16.475) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 135 thru_hole circle (at 29.4 -15.125) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 136 thru_hole circle (at 29.4 -13.775) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 137 thru_hole circle (at 29.4 -12.425) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 138 thru_hole circle (at 29.4 -11.075) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 139 thru_hole circle (at 29.4 -9.725) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 140 thru_hole circle (at 29.4 -8.375) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 141 thru_hole circle (at 29.4 -7.025) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 142 thru_hole circle (at 29.4 -5.675) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 143 thru_hole circle (at 29.4 -4.325) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 144 thru_hole circle (at 29.4 -2.975) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 145 thru_hole circle (at 31.3 -17.825) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 146 thru_hole circle (at 31.3 -16.475) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 147 thru_hole circle (at 31.3 -15.125) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 148 thru_hole circle (at 31.3 -13.775) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 149 thru_hole circle (at 31.3 -12.425) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 150 thru_hole circle (at 31.3 -11.075) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 151 thru_hole circle (at 31.3 -9.725) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 152 thru_hole circle (at 31.3 -8.375) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 153 thru_hole circle (at 31.3 -7.025) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 154 thru_hole circle (at 31.3 -5.675) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 155 thru_hole circle (at 31.3 -4.325) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 156 thru_hole circle (at 31.3 -2.975) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 157 thru_hole circle (at 33.2 -17.825) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 158 thru_hole circle (at 33.2 -16.475) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 159 thru_hole circle (at 33.2 -15.125) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 160 thru_hole circle (at 33.2 -13.775) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 161 thru_hole circle (at 33.2 -12.425) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 162 thru_hole circle (at 33.2 -11.075) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 163 thru_hole circle (at 33.2 -9.725) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 164 thru_hole circle (at 33.2 -8.375) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 165 thru_hole circle (at 33.2 -7.025) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 166 thru_hole circle (at 33.2 -5.675) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 167 thru_hole circle (at 33.2 -4.325) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 168 thru_hole circle (at 33.2 -2.975) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 169 thru_hole circle (at 35.1 -17.825) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 170 thru_hole circle (at 35.1 -16.475) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 171 thru_hole circle (at 35.1 -15.125) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 172 thru_hole circle (at 35.1 -13.775) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 173 thru_hole circle (at 35.1 -12.425) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 174 thru_hole circle (at 35.1 -11.075) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 175 thru_hole circle (at 35.1 -9.725) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 176 thru_hole circle (at 35.1 -8.375) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 177 thru_hole circle (at 35.1 -7.025) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 178 thru_hole circle (at 35.1 -5.675) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 179 thru_hole circle (at 35.1 -4.325) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 180 thru_hole circle (at 35.1 -2.975) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 181 thru_hole circle (at 37 -17.825) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 182 thru_hole circle (at 37 -16.475) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 183 thru_hole circle (at 37 -15.125) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 184 thru_hole circle (at 37 -13.775) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 185 thru_hole circle (at 37 -12.425) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 186 thru_hole circle (at 37 -11.075) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 187 thru_hole circle (at 37 -9.725) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 188 thru_hole circle (at 37 -8.375) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 189 thru_hole circle (at 37 -7.025) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 190 thru_hole circle (at 37 -5.675) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 191 thru_hole circle (at 37 -4.325) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 192 thru_hole circle (at 37 -2.975) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 193 thru_hole circle (at 38.9 -17.825) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 194 thru_hole circle (at 38.9 -16.475) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 195 thru_hole circle (at 38.9 -15.125) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 196 thru_hole circle (at 38.9 -13.775) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 197 thru_hole circle (at 38.9 -12.425) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 198 thru_hole circle (at 38.9 -11.075) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 199 thru_hole circle (at 38.9 -9.725) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 200 thru_hole circle (at 38.9 -8.375) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 201 thru_hole circle (at 38.9 -7.025) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 202 thru_hole circle (at 38.9 -5.675) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 203 thru_hole circle (at 38.9 -4.325) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 204 thru_hole circle (at 38.9 -2.975) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 205 thru_hole circle (at 40.8 -17.825) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 206 thru_hole circle (at 40.8 -16.475) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 207 thru_hole circle (at 40.8 -15.125) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 208 thru_hole circle (at 40.8 -13.775) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 209 thru_hole circle (at 40.8 -12.425) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 210 thru_hole circle (at 40.8 -11.075) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 211 thru_hole circle (at 40.8 -9.725) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 212 thru_hole circle (at 40.8 -8.375) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 213 thru_hole circle (at 40.8 -7.025) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 214 thru_hole circle (at 40.8 -5.675) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 215 thru_hole circle (at 40.8 -4.325) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 216 thru_hole circle (at 40.8 -2.975) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 217 thru_hole circle (at 42.7 -17.825) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 218 thru_hole circle (at 42.7 -16.475) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 219 thru_hole circle (at 42.7 -15.125) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 220 thru_hole circle (at 42.7 -13.775) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 221 thru_hole circle (at 42.7 -12.425) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 222 thru_hole circle (at 42.7 -11.075) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 223 thru_hole circle (at 42.7 -9.725) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 224 thru_hole circle (at 42.7 -8.375) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 225 thru_hole circle (at 42.7 -7.025) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 226 thru_hole circle (at 42.7 -5.675) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 227 thru_hole circle (at 42.7 -4.325) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 228 thru_hole circle (at 42.7 -2.975) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 229 thru_hole circle (at 44.6 -17.825) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 230 thru_hole circle (at 44.6 -16.475) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 231 thru_hole circle (at 44.6 -15.125) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 232 thru_hole circle (at 44.6 -13.775) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 233 thru_hole circle (at 44.6 -12.425) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 234 thru_hole circle (at 44.6 -11.075) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 235 thru_hole circle (at 44.6 -9.725) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 236 thru_hole circle (at 44.6 -8.375) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 237 thru_hole circle (at 44.6 -7.025) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 238 thru_hole circle (at 44.6 -5.675) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 239 thru_hole circle (at 44.6 -4.325) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad 240 thru_hole circle (at 44.6 -2.975) (size 0.8 0.8) (drill 0.39) (layers *.Cu *.Mask))
  (pad "" np_thru_hole circle (at 3.75 -6.405) (size 3.56 3.56) (drill 3.56) (layers *.Cu *.Mask))
  (pad "" np_thru_hole circle (at 49.35 -6.405) (size 3.56 3.56) (drill 3.56) (layers *.Cu *.Mask))
)